**korkment**

Korkment is a calendered compact underlayer in sheet, 2m wide, always used in combination with our DLW Linoleum compact Linoleum 2.0mm/2.50mm to reach a impact sound insulation of 15dB ( EN ISO 10140) for the total system.

Its weight is 1450gr/sqm and a total thickness of 2.00mm

Korkment is made from lineseed oil, resin,cork with a jute backing. It is is 100% recyclable and rated Cfl-s1 for fire resistance.

Designed and manufactured in a sustainable way in a plant awarded with ISO 9001 (quality), ISO 14001 (environment) and ISO 50001 (energy) certifications