#

**TARASTEP PRO** is an **heterogenous**, **sound-absorbing** solution with reinforced layer and transparent wearlayer, used to **recover indoor stairs in a single element**.

**TARASTEP PRO is an all-in-one** covering that covers the tread, the stair nosing - with a reinforced non-slip surface, and the riser.

It has a total thickness of 3.45 mm, with a **wear layer of 1 mm** which gives it great resistance to traffic and a residual indentation of 0.10 mm (value measured).

With a high-density foam backing, TARASTEP PRO provides 17dB of sound insulation and 63dB of walking noise.

**It complies with accessibility regulations**. The stair nosing specially designed to facilitate movement presents a **tactile contrast and a visual contrast** of at least 70% on each color.

**TARASTEP PRO** is suitable for premises classified **34/42 European class.**

According to standard NF EN 13501-1, the coating is classified Bfls1.

It is phthalate-free and complies with the European REACH regulation. TVOC air emissions at 28 days (NF EN 16000) of the selected coating are < 100 μg / m³.

It is 100% recyclable.